=======================================================================
Expedition PCB - Pinnacle - Version 2009.0.369.456
=======================================================================

Job Directory:        H:\job\SolidRun\CARRIER-ONE-rev2\PCB\

Design Status Report: H:\job\SolidRun\CARRIER-ONE-rev2\PCB\LogFiles\DesignStatus_11.txt

Sat Jan 11 20:23:05 2014

=======================================================================
DESIGN STATUS
=======================================================================
Board Size Extents  ............ 3.35 X 2.2 (in)
Route Border Extents  .......... 3.3 X 2.16 (in)
Actual Board Area  ............. 7.38 (in)
Actual Route Area  ............. 7.12 (in)

Placement Areas: Name            Available         Required          Required/Available
                 Entire Board    14.76 Sq. (in)    6.02 Sq. (in)     40.78 %

Pins  .......................... 899
Pins per Route Area  ........... 126.3 Pins/Sq. (in)

Layers  ........................ 4
    Layer 1 is a signal layer
        Trace Widths  .......... 5, 6, 8, 9, 10, 15, 20, 30
    Layer 2 is a Positive Plane Layer with nets
        GND
        GNDC
        Trace Widths  .......... 5, 20
    Layer 3 is a Positive Plane Layer with nets
        GND
        GNDC
        Trace Widths  .......... 20, 40
    Layer 4 is a signal layer
        Trace Widths  .......... 5, 6, 8, 9, 10, 20, 30

Nets  .......................... 200
Connections  ................... 645
Open Connections  .............. 0
Differential Pairs  ............ 41
Differential Pair Names:   CLK1_N   CLK1_P
                           CSI_CLK0M   CSI_CLK0P
                           CSI_D0M   CSI_D0P
                           CSI_D1M   CSI_D1P
                           CSI_D2M   CSI_D2P
                           CSI_D3M   CSI_D3P
                           DSI_CLK0M   DSI_CLK0P
                           DSI_D0M   DSI_D0P
                           DSI_D1M   DSI_D1P
                           HDMI_CLKM   HDMI_CLKP
                           HDMI_D0M   HDMI_D0P
                           HDMI_D1M   HDMI_D1P
                           HDMI_D2M   HDMI_D2P
                           LVDS0_CLK_N   LVDS0_CLK_P
                           LVDS0_TX0_N   LVDS0_TX0_P
                           LVDS0_TX1_N   LVDS0_TX1_P
                           LVDS0_TX2_N   LVDS0_TX2_P
                           LVDS1_CLK_NEG   LVDS1_CLK_POS
                           LVDS1_TX0_NEG   LVDS1_TX0_POS
                           LVDS1_TX1_NEG   LVDS1_TX1_POS
                           LVDS1_TX2_NEG   LVDS1_TX2_POS
                           MDI_TRXN0   MDI_TRXP0
                           MDI_TRXN1   MDI_TRXP1
                           MDI_TRXN2   MDI_TRXP2
                           MDI_TRXN3   MDI_TRXP3
                           N16787605   N16787608
                           N16787611   N16787614
                           N16796046   N16796048
                           PCIE_CREFCLKM   PCIE_CREFCLKP
                           PCIE_CRXM   PCIE_CRXP
                           PCIE_CTXM   PCIE_CTXP
                           PCIE_RXM   PCIE_RXP
                           PCIE_TXM   PCIE_TXP
                           SATA_RXN   SATA_RXP
                           SATA_TXN   SATA_TXP
                           USB_HOST_DN   USB_HOST_DP
                           USB_HUB_DN1   USB_HUB_DP1
                           USB_HUB_DN2   USB_HUB_DP2
                           USB_HUB_DN3   USB_HUB_DP3
                           USB_HUB_DN4   USB_HUB_DP4
                           USB_OTG_DN   USB_OTG_DP
                           
Percent Routed  ................ 100.00 %

Netline Length  ................ 0 (in)
Netline Manhattan Length  ...... 0 (in)
Total Trace Length  ............ 286.35 (in)

Trace Widths Used (th)  ........ 5, 6, 8, 9, 10, 15, 20, 30, 40
Vias  .......................... 618
Via Span  Name                   Quantity
   1-4    022VIA_10              618

Teardrops....................... 0
    Pad Teardrops............... 0
    Trace Teardrops............. 0
    Custom Teardrops............ 0
Breakouts....................... 0

Virtual Pins.................... 0
Guide Pins ..................... 0

Parts Placed  .................. 164
    Parts Mounted on Top  ...... 115
        SMD  ................... 104
        Through  ............... 11
        Test Points  ........... 0
        Mechanical  ............ 0
    Parts Mounted on Bottom  ... 49
        SMD  ................... 48
        Through  ............... 1
        Test Points  ........... 0
        Mechanical  ............ 0
    Embedded Components ........ 0
        Capacitors ............. 0
        Resistors .............. 0
    RF Shapes .................. 0

    Edge Connector Parts  ...... 0

Parts not Placed  .............. 0

Nested Cells  .................. 0

Jumpers  ....................... 0

Through Holes  ................. 715
    Holes per Board Area  ...... 96.91 Holes/Sq. (in)
Mounting Holes  ................ 14

Wirebonds
    Bondpads ................... 0
    Bond Wires ................. 0